[[1]](#footnote-1)

Advances in Battery Technology

Alyanna Y. Castillo, *UWEE*, Patrick G. Ma, *UWEE*, Ryan A. McDaniel, *UWEE*

*Abstract*—This paper will outline a few specific examples of the current advances in battery technology.  These examples will cover a few different types of organic batteries, flexible batteries, and supercapacitors.  Each of these has a different application for the future of electronic systems, ranging from electronic paper to waste water power management.  The applications of batteries is vast, and advancing battery technology beyond the bulky and heavy devices that are common now is essential for new electronics to become successful.

*Index Terms*— Advances, bacteria, battery, capacitors, electric cars, flexible, nanodot, nanoporous nickel-fluoride, StoreDot, supercapacitor.

# INTRODUCTION

B

atteries have become more and more important in the world of technology in the last few years.  The rise of smartphones in the consumer space made the demand for long-lasting batteries apparent.  High oil prices have shifted the focus of the automotive industry to efficient alternatives, like electrically powered vehicles.  Despite all of this demand, batteries are still the limiting factor in several revolutionary designs.

A typical battery is very large and bulky for the amount of energy it provides.  The designer of an electric car not only has to worry about carrying around the passengers, but also the immense weight of the batteries needed to power it.  The main contribution to the weight and thickness of a smartphone is the battery that powers it.  In addition, a battery has a very short lifespan.  An owner of a smartphone has no doubt complained about how they have to recharge their year-old phone halfway through the day.  Luckily, researchers have been looking into smaller, lighter, and longer lasting alternatives to the battery.  The first of which, is the supercapacitor.

# Supercapacitors

Supercapacitors are an alternative way of storing energy. Also known as ultracapacitors or double-layer capacitors, they differ from regular capacitors in that they have a very high capacitance. Energy is stored through static charge instead of an electrochemical reaction. Table 1 shows a chart comparing the performance of a supercapacitor to a Li-ion battery [1].

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Energy\* | Power\*\* | Life Cycle | Discharge Time |
| Battery | High | Low | Short | Slow |
| Super Capacitor | Low | High | Long | Fast |

# StoreDot

StoreDot is an Israeli company that plans to reinvent the battery using Quantum Dot technology [2].  Their specific trademark is called Nanodot, which is a small protein called a peptide that can hold an electric charge.  The company would sandwich these peptides between two dielectric sheets.  After placing an electrode on each sheet, the system would become a new type of supercapacitor.

StoreDot’s supercapacitor would have the advantages of both batteries and supercapacitors.  The capacitor would charge quickly and discharge slowly, and it could be recharged and discharged several times before losing capacity.  The problem with the nanodot capacitor right now is that the company has only created a prototype - and it is not even a consumer prototype.  Beginning mass production on this type of capacitor would be difficult as well, since it is a completely new method of storing energy.  There is still a lot of work to do for StoreDot, and their technology will have be be proven a bit more before it hits the mass market.

# Microbial Battery

The microbial battery was developed by a team at Stanford University.  They call it a Microbial Fuel Cell (MFC), and it uses exoelectrogens to generate electricity from sewage [3].  Exoelectrogens are a type of bacteria that evolved to emit electricity upon digestion of plant and animal waste.  These bacteria can be placed in a sample of waste water along with some kind of catalyst in order to store electricity.

Researchers at Stanford demonstrated the use of exoelectrogens by adding them to a sample of waste water along with some silver oxide (Fig. 1).  Two electrodes were attached to the container holding the waste water, and the team waited while the bacteria fed on all of the garbage in the liquid.  As the bacteria ate, the silver oxide would capture the electrons being emitted, which would cause the silver oxide to turn into silver metal and accumulate on the electrodes.  When the bacteria finishes eating, all the silver metal is taken out of the waste water and reoxidized to release the stored electricity.

The process described above would yield approximately 30% of energy that is contained in waste water.  This is actually a pretty good efficiency rating, considering solar panels also are only around 30% efficient.  However, there is much more solar energy out there than there is waste water energy.  The researchers hoped that this process could be used to offset the cost of waste water treatment, not necessarily power consumer electronics.  Microbial fuel cells have not been deployed in waste water plants yet.  The Stanford experiment was only a proof of concept, and in a real application silver oxide is too expensive to use as a catalyst.

# Flexible Batteries

As devices become smaller and more powerful, the need for smaller batteries increases. Flexible battery technology is a solution to this problem, since they do not have the same physical limits as lithium ion batteries or supercapacitors. These make them ideal for wearable computers and roll-up displays. Recently, flexible batteries are incorporated into RFID tags, smart cards, smart labels, and smart stickers. Smart stickers thermometers on packages of meat can track the temperatures of the product as it is being transported. Bus passesand credit cards can be electronic because flexible batteries can be placed in them without being bulky.

   Most flexible batteries share a similar appearance – they are essentially the Li-ion battery created with thin layers of each chemical. Energy is stored through electrochemical reactions between the different layers. However, there are various types of flexible batteries that are designed by different labs. For example, Blue Spark Technology specializes in disposable flexible batteries, which are commercially available. These non rechargeable batteries look like band aids and can be used in implantable medical devices.

The University of Illinois has a flexible lithium ion battery that can stretch but still retain charge, as shown in the image above. The battery is made up of tiny lithium ion cells which are connected by a network of silicon wires. The figure below shows a close up of how the cells are connected in these batteries [3]:

These silicon wires have a spring shape to them as shown above, allowing them to be stretched out and retain charge. Unlike Blue Spark’s batteries, these can be wirelessly recharged through induction.

Despite the physical advantages of flexible batteries, many still have the same problems as regular batteries, such as a low life cycle and low power density (kilo-watts/kg). Even high capacitance materials like lithium and graphene, which are used in high performance batteries, are generally brittle and difficult incorporate into flexible batteries.

Rice University’s flexible battery design has the advantages of a supercapacitor and a battery. Instead of lithium, they use a layer of nanoporous nickel-fluoride electrodes [5]. From the figure above, the structure is similar to a supercapacitor since the layers are of solid electrolytes instead of the liquid/gel electrolytes used in most flexible batteries [6]. However, it behaves like a battery through its electrochemical reactions for storing energy. The nano-sized pores in the nickel layer give more flexibility than lithium, allowing the battery to retain its supercapacitor/battery qualities even after being flexed 1000 times.  Below is a table comparing the characteristics of Rice’s flexible battery to a supercapacitor and a Li-ion battery:

|  |  |  |
| --- | --- | --- |
| Type | Energy Density\* | Power Density\*\* |
| Li-On Battery | 200 | 0.005-0.4 |
| Supercapacitor | 5-25 | 10-100 |
| Ni-Flex Battery | 384 | 112 |

From the table, the flexible battery has the energy density of a Li-ion battery, but retains the power density of a supercapacitor. Though further research is required to develop a manufacturing process for these batteries, these seem to be the ideal design for flexible batteries.

# Future

The commercial needs of products will be the largest driver of future battery development. As a result of this commercial driving force, the field of battery technology will diversify to match the needs of the devices and machines which use it. Since the consumer electronics industry was the first adopter of battery technology, some of the biggest steps forward have come about as a result of the need for batteries that combine lightweight, moderate power, and increasingly longer capacity batteries. Battery companies are trying to make batteries that are lighter, faster charging and flexible.

With the increased viability of ultra portable medical devices, manufacturers have to add to the existing consumer battery technology. Not only must batteries be lightweight, but now they must be a fraction of the size. Already battery technology can print batteries of the tiniest proportions. Expect future batteries to become even more compact and unobtrusive.

At the other end of the spectrum, automobile manufacturers are focusing heavily on electric vehicles. This demanding batteries capable of very high power capacities and the ability to deliver moderately high currents. weight is less of an issue, but minimization is still important. In this area of battery development, the use of more efficient nanocrystals and other lithium manufacturing techniques may become a significant factor. Improvements here are expected to deliver cars with gas milage beyond 1000 miles per gallon.

Large scale power has also begun to place demands on batteries. These batteries would be used to store massive amounts of energy --and deliver large amounts of current and voltage. Weight is a non-issue in this area, but the difficulty lies in creating efficient batteries able to deliver such large amounts of power quickly and store excess power as production and demand fluctuate. Being capable of capturing power from intermittent renewable energy sources and outputting clean power is a major factor in development for this field of electrical engineering. Recently, several companies such as Aquion Energy and Sumitomo have announced batteries designed specifically for large-scale power grids. It is reasonable to expect large-scale power batteries to form the basis for power management and energy storage in future power grids.

# Conclusion

As the technology we rely on becomes more and more advanced, the demands on batteries to meet our energy needs increases. With more fields of electrical engineering looking for consistent or portable power delivery, battery research has begun to increase. A single solution is no longer possible to address the diverse needs of each industry.

In addition to continued research in existing technologies, new approaches to batteries have shown commercial promise. In particular, supercapacitor-like batteries such as StoreDot and bio-chemical microbial alternatives show promise to revolutionize how are batteries viewed at large. Flexible and printable batteries are opening new avenues and markets for existing products and allowing the creation of devices which recently existed as only concepts. The research and concepts of today are quickly becoming the reality of tomorrow.

1. publication in a TRANSACTIONS or JOURNAL.

# Conclusion

A conclusion section is not required. Although a conclusion may review the main points of the paper, do not replicate the abstract as the conclusion. A conclusion might elaborate on the importance of the work or suggest applications and extensions.

Acknowledgment

The preferred spelling of the word “acknowledgment” in American English is without an “e” after the “g.” Use the singular heading even if you have many acknowledgments. Avoid expressions such as “One of us (S.B.A.) would like to thank ... .” Instead, write “F. A. Author thanks ... .” **Sponsor and financial support acknowledgments are placed in the unnumbered footnote on the first page.**

References

[1] AquionEnergy, “*S10 Battery Stack for Stationary, Long-Duration Applications*.” [Online]. Available: <http://www.aquionenergy.com/energy-storage-battery>. [Accessed: 04-May-2014].

[2] “*Lithium-based Batteries Information – Battery University.*” [Online]. Available: http://batteryuniversity.com/learn/article/lithium\_based\_batteries. [Accessed: 03-May-2014].

[3] “*Israeli company develops bio-organic LED displays to compete with OLEDs*.” [Online]. Available: http://www.oled-info.com/israeli-company-develops-bio-organic-led-displays-compete-oleds. [Accessed: 06-May-2014].

[4] “*Stanford scientists use ‘wired microbes’ to generate electricity from sewage.*”[Online]. Available: http://www.eurekalert.org/pub\_releases/2013-09/ssoe-ssu091113.php. [Accessed: 06-May-2014].

[5] S. Xu, Y. Zhang, and J. Cho, “*Stretchable batteries with self-similar serpentine interconnects and integrated wireless recharging systems*,” *Nature Publishing Group*, vol. 4, Feb. 2013.

[6] M. Williams, “*Flexible battery, no lithium required,*” 28-Apr-2014. [Online]. Available: http://news.rice.edu/2014/04/28/flexible-battery-no-lithium-required/. [Accessed: 04-May-2014].

[7]   P. Detwiler, "*Imergy: A Novel Vanadium Electrolyte Storage Technology*." Forbes, [Online serial], 2014 Apr 30 [2014 May 6]. Available: http://www.forbes.com/sites/peterdetwiler/2014/04/30/imergy-a-novel-vanadium-electrolyte-storage-technology/.

[8] Y. Yang, G. Ruan, G. Wang, and J. M. Tour, “*Flexible Three-Dimensional Nanoporous Metal-Based Energy Devices.*” Journal of the American Chemical Society, 30-Apr-2014. [Accessed: 04-May-2014]

**First A. Author** (M’76–SM’81–F’87) and the other authors may include biographies at the end of regular papers. Biographies are often not included in conference-related papers. This author became a Member (M) of IEEE in 1976, a Senior Member (SM) in 1981, and a Fellow (F) in 1987. The first paragraph may contain a place and/or date of birth (list place, then date). Next, the author’s educational background is listed. The degrees should be listed with type of degree in what field, which institution, city, state or country, and year degree was earned. The author’s major field of study should be lower-cased.

The second paragraph uses the pronoun of the person (he or she) and not the author’s last name. It lists military and work experience, including summer and fellowship jobs. Job titles are capitalized. The current job must have a location; previous positions may be listed without one. Information concerning previous publications may be included. Try not to list more than three books or published articles. The format for listing publishers of a book within the biography is: title of book (city, state: publisher name, year) similar to a reference. Current and previous research interests ends the paragraph.

The third paragraph begins with the author’s title and last name (e.g., Dr. Smith, Prof. Jones, Mr. Kajor, Ms. Hunter). List any memberships in professional societies other than the IEEE. Finally, list any awards and work for IEEE committees and publications. If a photograph is provided, the biography will be indented around it. The photograph is placed at the top left of the biography. Personal hobbies will be deleted from the biography.

1. Manuscript received October 9, 2001. (Write the date on which you submitted your paper for review.) This work was supported in part by the U.S. Depart­ment of Com­merce under Grant BS123456 (sponsor and financial support acknowledgment goes here). Paper titles should be written in uppercase and lowercase letters, not all uppercase. Avoid writing long formulas with subscripts in the title; short formulas that identify the elements are fine (e.g., "Nd–Fe–B"). Do not write "(Invited)" in the title. Full names of authors are preferred in the author field, but are not required. Put a space between authors' initials.

   F. A. Author is with the National Institute of Standards and Technology, Boulder, CO 80305 USA (corresponding author to provide phone: 303-555-5555; fax: 303-555-5555; e-mail: author@ boulder.nist.gov).

   S. B. Author, Jr., was with Rice University, Houston, TX 77005 USA. He is now with the Department of Physics, Colorado State University, Fort Collins, CO 80523 USA (e-mail: author@lamar. colostate.edu).

   T. C. Author is with the Electrical Engineering Department, University of Colorado, Boulder, CO 80309 USA, on leave from the National Research Institute for Metals, Tsukuba, Japan (e-mail: author@nrim.go.jp). [↑](#footnote-ref-1)